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INTERNAL STRUCTURE COMPOSITION
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RIGOROUS PRODUCTION PROCESS
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Operation Guidelines

Iy \o Pre-start Check Oil & Water Level
&

é Ensure oil and water levels are within the
6 specified range before starting.

Monitor Operating

Data During Operation

Keep an eye on voltage,
2nn frequency, and
temperature while the

generator is running.

Regular Maintenance
After Shutdown

Perform scheduled maintenance and cleaning after
each use for optimal performance.
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Reliable Outdoor Power
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Ideal For Outdoor

Construction

Stable Operation In Rain, Dust
& Extreme Temperature
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NOISE LEVEL COMPARISON

| Our Generator:
<70dB 70dB, No Disturbance
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APPLICATION SCENARIOS

4 No backup power means helplessness
emergency power supply to solve your problems

power supply for Hower supply Top
high-speed NS gonstruction sitd

power supply for mine
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Power For
Construction Sites

Reliable Electricity Supply
For Building Projects
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Genset Model Prime | Standby ésr’,m‘ Lm‘%:,‘ (%ﬁer : sumplior Amfﬁ}w S /pe w%:,}n
kW | KVA | KW | kVA KG

GF-TT-22 4B3.9-G11 i ! QK184ES 2200 x 900 x 1250
GF-TT-30 2 27 24 30 4B3.9-G1 4L 39 74 QK184F 2200x900x 1250 1150
GF-TT-30 22 27 24 30 4B3.9-G2 4L 3.9 6.7 QK184F 2200x900x 1250 1150
GF-TT-33 24 30 26 33 4B3.9-G12 aL 39 8 QK184G 2250 x 1000 x 1250 1200
GF-TT-44 32 40 36 44 4BT3.9-G1 4L 3.9 10 QK184G 2250 x 1000 x 1500 1230
GF-TT-44 32 40 36 44 4BT3.9-G2 aL 3.9 9.3 QK184J 2250 x 1000 x 1500 1230
GF-TT-55 40 50 44 55 4BTA3.9-G2 aL 3.9 1.5 QK184J 2350 x 1000 x 1500 1340
GF-TT-66 48 60 53 66 4BTA3.9-G2 aL 3.9 11:5; QK224D 2450 x 1000 x 1550 1400
GF-TT-86 64 80 70 88 4BTA3.9-G11 aL 3.9 20.1 QK224E 2450 x 1000 x 1500 1400
GF-TT-100 72 90 80 100 6BT5.9-G1 6L 59 22 QK224G 3000x 1100 x 1600 1683
GF-TT-110 80 100 88 110 6BT5.9-G2 6L 5.9 22 QK274C 3000x 1100 x 1600 1683
GF-TT-132 96 120 106 132 6BTA5.9-G2 6L 59 27 QK274C 3000x 1100 x 1600 1700
GF-TT-150 110 138 121 151 6BTAA5.9-G2 6L 5.9 30 QK274D 3100x 1100 x 1600 1810
GF-TT-180 130 163 143 179 6BTAA5.9-G12 6L 59 325 QK274E 3100x1100x 1650 1894
GF-TT-200 150 188 165 206 B6CTA8.3-G1 6L 8.3 42 QK274F 3250x 1120 x 1850 2393
GF-TT-200 150 188 165 206 6CTAB.3-G2 6L 8.3 42 QK274F 3250x 1120 x 1850 2393
GF-TT-220 160 200 176 220 B6CTAAB.3-G2 6L 8.3 45.4 QK274H 3300 x 1200 x 1850 2350
GF-TT-275 200 250 220 275 6LTAAB.9-G2 6L 89 53 QK274H 3600 x 1250 x 1900 2450
GF-TT-290 210 263 231 290 6LTAA8.9-G3 6L 8.9 53 QK314D 3700 x 1250 x 1900 2887
GF-TT-350 254 318 280 350 6LTAA9.5-G1 6L 9.5 70 QK314E 3700x 1250 x 1900 2900
GF-TT-400 288 360 320 400 QSZ13-G6 6L 13 81 QK314F 4400 x 1700 x 2390 4350
GF-TT-413 300 375 330 413 B6ZTAA13-G3 6L 13 79 QK314F 4400 x 1700 x 2390 4350
GF-TT-440 320 400 352 440 QSZ13-G7 6L 13 85 QK354C 4400 x 1700 x 2390 4350
GF-TT-480 350 438 384 480 B6ZTAA13-G2 6L 13 90 QK354C 4500 x 1700 x 2390 4420
GF-TT-480 350 438 384 480 B6ZTAA13-G4 6L 13 98 QK354C 4500 x 1700 x 2390 4420
GF-TT-480 350 438 384 480 QSZ13-G2 6L 13 70 QK354C 4500 x 1700 x 2390 4520
GF-TT-500 360 450 400 500 QSZ13-G5 6L 13 108 QK354C 4500 x 1700 x 2390 4520
GF-TT-550 400 500 440 550 QSZ13-G3 6L 13 102 QK354D 4500 x 1700 x 2390 4520
GF-TT-275 200 250 220 275 MTA11-G2 6L 10.8 49.9 QK274K 3750 x 1400 x 2100 3700
GF-TT-275 200 250 220 275 NT855-GA 6L 13 53 QK274K 3900 x 1400 x 2100 3785
GF-TT-275 200 250 220 275 NTA855-G1 6L 14 67.6 QK274K 3900 x 1400 x 2100 3850
GF-TT-303 220 275 242 303 NTA855-G1A 6L 14 61.3 QK314D 3950 x 1400 x 2100 3950
GF-TT-344 250 313 275 344 MTAA11-G3 6L 10.8 62 QK314E 3950 x 1450 x 2100 4000
GF-TT-344 250 313 275 344 NTA855-G1B 6L 14 64.9 QK314E 3950 x 1400 x 2100 4000
GF-TT-344 250 313 275 344 NTA855-G2 6L 14 61 QK314E 3950 x 1400 x 2100 4000
GF-TT-378 275 344 303 378 NTA855-G2A 6L 14 71.9 QK314F 4200 x 1400 x2100 4200
GF-TT-385 280 350 308 385 NTA855-G4 6L 14 75.3 QK314F 4200 x 1400 x 2100 4200
GF-TT-413 300 375 330 413 NTAA855-G7 6L 14 85.4 QK314F 4300 x 1450 x 2250 4350
GF-TT-413 300 375 330 413 KTA19-G2 6L 19 83 QK314F 4450 x 1700 x 2450 4650
GF-TT-440 320 400 352 440 QSNT-G3 6L 14 84.2 QK354C 4500 x 1700 x 2390 4800
GF-TT-440 320 400 352 440 NTAAB55-G7A 6L 14 89.2 QK354C 4400 x 1450 x 2250 4400
GF-TT-500 360 450 400 500 KTA19-G3 6L 19 97 QK354C 4500 x 1700 x 2450 4800
GF-TT-550 400 500 440 550 KTA19-G3A 6L 19 107 QK354D 4500 x 1700 x 2450 4800
GF-TT-550 400 500 440 550 KTA19-G4 6L 19 107 QK354D 4500 x 1700 x 2500 4900
GF-TT-578 420 525 462 578 KTAA19-G5 6L 19 113 QK354E 4800 x 1800 x 2500 5500
GF-TT-633 460 575 506 633 KTAA19-G6 6L 19 118.5 QK354E 4800 x 1800 x 2500 5500
GF-TT-650 472 590 520 650 KTA19-G8 6L 19 144 QK354E 4800 x 1800 x 2500 5600
GF-TT-715 520 650 572 715 QSK19-G4 6L 18.9 147 QK354F 20GP 6610
GF-TT-688 500 625 550 688 KTAA19-G6A 6L 19 149.5 QK354F 4900 x 1800 x 2500 5800
GF-TT-688 500 625 550 688 KT38-G vi2 38 140 QK354F 20HC 8400
GF-TT-788 570 713 630 788 KT38-G1 vi2 38 140 QK404C 20HC 8500
GF-TT-800 580 725 640 800 KT38-GA vi2 38 158 QK404C 20HC 8550
GF-TT-825 600 750 660 825 KTA38-G2 vi2 38 167 QK404C 20HC 8600
GF-TT-880 640 800 704 880 KTA38-G2B vi2 38 170 QK404D 20HC 8700
GF-TT-1000 728 910 800 1000 KTA38-G2A vi2 38 191 QK404E 20HC 8850
GF-TT-1100 800 1000 880 1100 KTA38-G5 vi2 38 209 QK404F 40HC 11150
GF-TT-1250 900 1125 1000 1250 KTA38-G9 vi2 38 256 QK404G 40HC 11210
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QUIET OPERATION =65dB
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Strict Manufacturing Process

High prmperature Core Components Performance Testing
Assembly
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ULTRA-QUIET INDUSTRIAL GENERATOR

Reliable Power Supply for All Scenarios
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Premium Detail Design

Slent canopy
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Industrial Muffler

Emergency Stop Button
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3 CORE ADVANTAGES
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WATERPROOF &
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<70dB
ULTRA QUIET
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Internal Material Composition

Thickened High Temperature  Perforated Sound Flame Retardant
Galvanized Steel Spray Coating Absorbing Panel  Sound Absorbing Cotton

Flame Retardant
Sound Absorbing
Cotton

Water Cooled
Diesel Engine

Flame Retardant
Sound Absorbing Cotton




