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INTERNAL STRUCTURE COMPOSITION
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RIGOROUS PRODUCTION PROCESS

PRECISION WELDING

IP22 SEALING TEST
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Operation Guidelines

Iy \C) Pre-start Check Oil & Water Level
4

é Ensure oil and water levels are within the
6 specified range before starting.

Monitor Operating

Data During Operation

Keep an eye on voltage,
2nn frequency, and
temperature while the

generator is running.

Regular Maintenance
After Shutdown

Perform scheduled maintenance and cleaning after
each use for optimal performance.
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Reliable Outdoor Power
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Ideal For Outdoor
Construction

Stable Operation In Rain, Dust
& Extreme Temperature
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NOISE LEVEL COMPARISON
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| Our Generator:
<70dB 70dB, No Disturbance
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APPLICATION SCENARIOS

4 No backup power means helplessness
emergency power supply to solve your problems

power supply fo

high-speed jiéins power supply for mine
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Power For
Construction Sites

Reliable Electricity Supply
For Building Projects





image1.jpeg
(G CANANAY
==/ 5PRINGIR

MRS MAZBANZE  50HZ/1500RPM
CANAAN SPRING Diesel Generator Set

WA= P AR &R
nans *Gansm output Y:.rhn‘n' u rit :Umss! Engine e -
kW | kVA | kW | kVA = [ L/h mm KG

GF-TT-25 18 225 20 25 WP2.3D25E200 aL 2.289 6.09 QK184E 1950 x 850 x 1100 730
GF-TT-35 258 1311 2281 N335 WP2.3D33E200 4L 2.289 8.1 QK184G 1950 x 850 x 1100 880
GF-TT-41 30 375 33 41 WP2.3D40E200 4L 23 97 QK184H 2050x850% 1100 1165
GF-TT-50 36 45 40 50 WP2.3D48E200 aL 23 11.9 QK224D 2250x950x 1250 1230
GF-TT-70 50 625 56 70 WP4.1D66E200 aL 4.09 16.9 QK224E 2550x 1000 x 1300 1245
GF-TT-88 64 80 70 88 WP4.1D80E200 4L 4.09 20.3 QK224G 2600x 1000x 1300 1730
GF-TT-110 80 100 88 110 WP4.1D100E200 4L 4.5 22 QK274C 2800x 1050 x 1600 1760
GF-TT-138 100 125 110 138 WP6D132E200 6L 6.75 29.6 QK274E 3250 x 1100 x 1600 1870
GF-TT-165 120 150 132 165 WP6D152E200 6L 6.75 34 QK274F 3350x1100x 1600 1890
GF-TT-180 130 162.5 144 180 WP6D167E200 6L 6.75 375 QK274F 3400x1100x 1600 1910
GF-TT-206 150 187.5 165 206 WP10D200E200 6L 9.726 471 QK274H 3700x 1300 x 1800 1950
GF-TT-250 180 225 200 250 WP10D238E200 6L 9.726 55.9 QK274J 3800x 1300x 1800 2680
GF-TT-275 200 250 220 275 WP10D264E200 6L 9.726 62.1 QK274K 3800x1300x 1800 2750
GF-TT-344 250 3125 275 344 WP10D320E200 6L 9.726 733 QK314E 3900 x 1300 x 1800 3100
GF-TT-344 250 312.5 275 344 WP12D353E200 6L 11.596 72.8 QK314E 4100 x 1600 x 2250 4120
GF-TT-413 300 375 330 413 WP13D385E200 6L 12.54 63.2 QK314F 4200 x 1600 x 2250 5710
GF-TT-450 330 412.5 360 450 WP13D405E200 6L 12.54 93.1 QK354C 4300x 1600 % 2250 5770

GF-TT-495 360 450 396 495 WP13D440E310 6L 12,54 101.2 QK354C 4300 x 1600 x 2250 5800
GF-TT-550 400 500 440 550 WP13D490E311 6L 15.9 11.3 QK354D 4500 x 1800 x 2500 6020

GF-TT-633 460 575 506 633  6M33D633E200 6L 19.6 131.5 QK354E 4500 x 2000 x 2500 6560
GF-TT-725 520 650 580 725  6M33D633E200 6L 19.6 145.4 QK354F 4650 x 2000 x 2500 15200
GF-TT-750 550 688 600 750 6M33D670E200 6L 19.6 154.3 QK354F 4800 x 2000 x 2500 16500
GF-TT-825 600 750 660 825  6M33D725E200 6L 20 165 QK404C 4800 x 2000 x 2500 16800
GF-TT-880 640 800 704 880 12M26D792E200 V12  31.8 1821 QK404D 20GP 17300
GF-TT-990 720 900 792 990 12M26D902E200 V12 31.8 207.4 QK404E 20GP 17820
GF-TT-1100 800 1000 880 1100 12M26D968E200 V12 31.8 222.65 QK404F 20GP 17860
GF-TT-1238 900 1125 990 1238 12M33D1108E200 V12  39.2 254.7 QK404G 40HC 18450
GF-TT- 1375 1000 1250 1100 1375 12M33D1210E200 V12  39.2 278.3 QK404H 40HC 18500

GF-TT-1500 \ \ 1200 1500 12M33D1320E200 V12 39.2 303.6 QK454B 40HC 18900
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QUIET OPERATION =65dB
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Strict Manufacturing Process

High prmperature Core Components Performance Testing
Assembly

CEIS39001

LTRA-QUIET INDUSTRIAL GENERATOR

Reliable Power Supply for All Scenarios





image4.jpeg
Premium Detail Design

Slent canopy
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Industrial Muffler

Emergency Stop Button
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3 CORE ADVANTAGES
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WATERPROOF &
DUSTPROOF

<70dB
ULTRA QUIET

=S +1%
‘ VOLTAGE STABILITY
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Internal Material Composition

Thickened High Temperature  Perforated Sound Flame Retardant
Galvanized Steel Spray Coating Absorbing Panel  Sound Absorbing Cotton

Flame Retardant
Sound Absorbing
Cotton

Water Cooled
Diesel Engine

Flame Retardant
Sound Absorbing Cotton




